DISPLAY:<ESC>[4;36HVAX?<ESC>[24;1H
TIMER:5
SEND: CALL<CR>
NO SKIP ON:ENTER NUMBER:
SKIP:25
SEND: CALL<CR>
NO SKIP ON:ENTER NUMBER:
SKIP:22
SEND: CALL<CR>
NO SKIP ON:ENTER NUMBER:
SKIP:19

DTR CLEAR:
DISPLAY:<ESC>[5;24r<ESC>[24;1H<CTRL/G><CTRL/G><CTRL/G><CR><LF><LF><LF>
DISPLAY:<ESC>[1m
DISPLAY:                       ** Communications failure **<CR><LF>
DISPLAY:<ESC>[0m<CR><LF>
DISPLAY:        After the 'CALL, DISPLAY, or MODIFY' message was <CR><LF>
DISPLAY:        displayed, a  CALL  was attempted.  However, the Rolm <CR><LF>
DISPLAY:        system did not respond with an 'ENTER NUMBER:' prompt as <CR><LF>
DISPLAY:        expected.  This may indicate that there is some problem <CR><LF>
DISPLAY:	problem with the Rolm system.<CR><LF>
DISPLAY:                        Please try a second time!<CR><LF>
DISPLAY:<CR><LF>
DISPLAY:        If it still does not respond, report the problem to the <CR><LF>
DISPLAY:        Information Center Help desk at: <CR><LF><LF>
DISPLAY:                              <ESC>[1m(313) 555-HELP<ESC>[0m<CR>
PAUSE:18
TIMEOUT:

PAUSE:2
DISPLAY:<ESC>[4;36H<ESC>[1m

