# Virtual Network Computing from ORL |

|  | ## VNCviewer for Windows CE 2.x Note: This should be considered a beta release. Use at your own risk! Now you can view X Windows applications on your PDA! This initial release of the VNC viewer for Windows CE is based heavily on the Win32 viewer. Most of the command-line arguments and options are taken directly from there, and you should look at the Windows viewer documentation for more details. The viewer requires Windows CE 2.0 or later. To install, make sure that TCP/IP is working correctly on your WinCE machine (try browsing the web) and I suggest you set the communications link to the fastest speed it can manage. I suggest you try connecting to the smallest desktop you can, initially. If you're viewing a PC or Mac, set the server's screen to 640x480 or so and 256 colours. If you're connecting to an Xvnc server, then you can of course create a desktop of any size you like. Larger screens will work - I've viewed a 1280x1024x24 screen here, but the initial screen download takes quite a while, and in this version a copy of the entire remote screen is kept in the PDA's memory, so make sure you've got plenty of RAM free! Copy the appropriate vncview.exe binary onto the PDA and run it. If you have used the Windows viewer the dialogs and menus should look very familiar. You might want to use the Options button in the Connection dialog to request 8-bit pixels only. You can set this from the command line, so I suggest you create a shortcut to the vncview executable and include the '-8bit' option in the target command line. The Windows CE viewer does not operate in full-screen or listening mode. There is no console-mode debugging, and some of the other Win32 viewer options are not implemented.. This is certainly the smallest X terminal I've ever used! go back to documentation |
For comments, feedback, etc, please see the 'Keeping in touch' page. Copyright 1998 - The Olivetti & Oracle Research Lab