 MODIFIED BY R. VENHOLA, 22-JUN-1988 VERSION 4.0

	1. FIXED A BUG WHEN COPYING TAPES THAT START WITH AN EOF MARK : THE
	   PROGRAM WOULD NOT WRITE OUT THE EOF MARK, BUT SKIP IT AND START
	   WRITING RECORDS
	2. ADDED A CHECK FOR BATCH MODE
	3. ON A PARITY ERROR IN BATCH THE PROGRAM NOW CONTINUES
	4. FINAL MENU EXPANDED TO HANDLE FIFTH OPTION OF WRITING TWO EOFS
	   TO THE OUTPUT TAPE AS SOME OF OUR DATA TAPES LACK PROPER EOFS
	5. CHANGED DEFAULT DEVICES (INPUT MSA0:, OUTPUT MFA0:)

 NOTE TWO NEW SUBROUTINES WERE ADDED IN SECTION `E'
